(footprint "pin_header_127_8pin" (version 20221018) (generator opencad-lib)
  (layer "F.Cu")
  (descr "Pin Header 1.27mm 1.27mm 8-pin THT vertical. Dimensions match KiCad official Connector_JST (datasheet-derived).")
  (tags "Pin Header 1.27mm connector 1.27mm 8pin")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.445 -2.110) (layer "F.SilkS"))
  (fp_text value "pin_header_127_8pin" (at 4.445 2.110) (layer "F.Fab"))
  (pad "1" thru_hole roundrect (at 0 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25))
  (pad "2" thru_hole oval (at 1.270 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole oval (at 2.540 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole oval (at 3.810 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole oval (at 5.080 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole oval (at 6.350 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole oval (at 7.620 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole oval (at 8.890 0) (size 1.0 1.0) (drill 0.65) (layers "*.Cu" "*.Mask"))
)
