(footprint "jst_xh_2pin" (version 20221018) (generator opencad-lib)
  (layer "F.Cu")
  (descr "JST XH 2.5mm 2-pin THT vertical. Dimensions match KiCad official Connector_JST (datasheet-derived).")
  (tags "JST XH connector 2.5mm 2pin")
  (attr through_hole)
  (fp_text reference "REF**" (at 1.250 -3.460) (layer "F.SilkS"))
  (fp_text value "jst_xh_2pin" (at 1.250 4.510) (layer "F.Fab"))
  (pad "1" thru_hole roundrect (at 0 0) (size 1.7 2.0) (drill 1.0) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25))
  (pad "2" thru_hole oval (at 2.500 0) (size 1.7 2.0) (drill 1.0) (layers "*.Cu" "*.Mask"))
)
