(footprint "jst_xh_3pin" (version 20221018) (generator opencad-lib)
  (layer "F.Cu")
  (descr "JST XH 2.5mm 3-pin THT vertical. Dimensions match KiCad official Connector_JST (datasheet-derived).")
  (tags "JST XH connector 2.5mm 3pin")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.500 -3.460) (layer "F.SilkS"))
  (fp_text value "jst_xh_3pin" (at 2.500 4.510) (layer "F.Fab"))
  (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25))
  (pad "2" thru_hole oval (at 2.500 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole oval (at 5.000 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask"))
)
