(footprint "yeonho_smw250_03p"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Yeonho SMW250-03 wire-to-board wafer 3P straight, pitch 2.5mm, AC/DC 250V 3A, body 9.9x5.8x7.0mm, pin sq0.64, drill 1.0, hole span 5.0. Pin row offset: LOCK front 3.45 / back 2.35 (datasheet PCB LAYOUT)")
	(tags "connector wafer Yeonho SMW250 2.5mm 3P straight")
	(attr through_hole)
	(property "Reference" "J**"
		(at 2.50 -3.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "SMW250-03"
		(at 2.50 6.0 0)
		(layer "F.Fab")
	)
	(property "Datasheet" "" (at 0 0 0) (layer "F.Fab") (hide yes))
	(property "Description" "Yeonho SMW250 wafer 3P 2.5mm straight" (at 0 0 0) (layer "F.Fab") (hide yes))
	(pad "1" thru_hole rect (at 0.00 0) (size 1.7 1.7) (drill 1.0) (layers "*.Cu" "*.Mask"))
	(pad "2" thru_hole circle (at 2.50 0) (size 1.7 1.7) (drill 1.0) (layers "*.Cu" "*.Mask"))
	(pad "3" thru_hole circle (at 5.00 0) (size 1.7 1.7) (drill 1.0) (layers "*.Cu" "*.Mask"))
	(embedded_fonts no)
)
