(footprint "D_LCC-2A"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.1 -1.68 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "D_LCC-2A"
		(at -3.12 2.58 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.0095 -0.01 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0.0095 -0.01 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.12 3.78 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.12 4.98 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.12 6.18 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0.062 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0.01 0 0)
		(layer "User.9")
	)
	(pad "1" smd roundrect
		(at -1.8225 0)
		(size 1.525 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at 1.8225 0)
		(size 1.525 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "antmicro_1n5806u01a.glb"
		(offset
			(xyz 0.35 -0.29 2.05)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 0)
		)
	)
)
