(footprint "LED_RGY_1.6x1.6mm_APTF1616"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "1.6 x 1.6 mm Full-Color Surface Mount LED")
	(tags "LED")
	(property "Reference" "REF**"
		(at 0 -1.2 180)
		(layer "F.SilkS")
	)
	(property "Value" "LED_RGY_1.6x1.6mm_APTF1616"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.3 3.297 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.3 4.496 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.3 5.698 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.874 -0.499 270)
		(size 0.5 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.874 -0.499 270)
		(size 0.5 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.874 0.498 270)
		(size 0.5 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.874 0.498 270)
		(size 0.5 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_aptf1616surkcgksykc.glb"
		(offset
			(xyz -0.024 0.001 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
