(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LED_RGY_0606_APTF1616SURKCGKSYKC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LED_RGY_0606_APTF1616SURKCGKSYKC"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LED_RGY_0606_APTF1616SURKCGKSYKC"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.kingbrightusa.com/images/catalog/SPEC/APTF1616SURKCGKSYKC.pdf"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LED, RGY, SMD, 0606, R 30 mA, G 30 mA, Y 30 mA, R 1.95 V, G 2.1 V, Y 2 V, Common Anode"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "APTF1616SURKCGKSYKC"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Kingbright"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Color" "R, G, Y"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIODE, SEMICONDUCTOR, LED"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LED_RGY_0606_APTF1616SURKCGKSYKC_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 19.05 3.81 180)
					(length 2.54)
					(name "C_{R}")
					(number "2")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(name "C_{G}")
					(number "3")
				)
				(pin passive line
					(at 19.05 -3.81 180)
					(length 2.54)
					(name "C_{Y}")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
