(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LED_RGB_PLCC6_ASMB-TTF0-0A20B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LED_RGB_PLCC6_ASMB-TTF0-0A20B"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LED_RGB_PLCC6_ASMB-TTF0-0A20B"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.broadcom.com/doc/ASMB-TTF0-0A20B-DS101"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LED, RGB, SMD, PLCC-6, R 50 mA, G 30 mA, B 30 mA, R 2.1 V, G 2.9 V, B 2.9 V"
				(at 27.94 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ASMB-TTF0-0A20B"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Broadcom"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Color" "R, G, B"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIODE, SEMICONDUCTOR, LED, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LED_RGB_PLCC6_ASMB-TTF0-0A20B_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "A_{R}")
					(number "1")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(name "C_{R}")
					(number "2")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(name "A_{G}")
					(number "3")
				)
				(pin passive line
					(at 19.05 -3.81 180)
					(length 2.54)
					(name "C_{G}")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A_{B}")
					(number "5")
				)
				(pin passive line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "C_{B}")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
