(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BQ24735"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BQ24735"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BQ24735"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24735.pdf?ts=1723124445323"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1- to 4-Cell Li+ Battery SMBus Charge Controller for Supporting Turbo\nBoost Mode With N-Channel Power MOSFET Selector"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BQ24735"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, MANAGEMENT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BQ24735_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "ACN")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "ACP")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CMSRC")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "ACDRV")
					(number "4")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 2.54)
					(name "ACOK")
					(number "5")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "ACDET")
					(number "6")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 2.54)
					(name "IOUT")
					(number "7")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SDA")
					(number "8")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SCL")
					(number "9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ILIM")
					(number "10")
				)
				(pin passive line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "BATDRV")
					(number "11")
				)
				(pin passive line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "SRN")
					(number "12")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 2.54)
					(name "SRP")
					(number "13")
				)
				(pin power_in line
					(at 27.94 -45.72 180)
					(length 2.54)
					(name "GND")
					(number "14")
				)
				(pin passive line
					(at 27.94 -30.48 180)
					(length 2.54)
					(name "LODRV")
					(number "15")
				)
				(pin passive line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "REGN")
					(number "16")
				)
				(pin passive line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "BTST")
					(number "17")
				)
				(pin passive line
					(at 27.94 -20.32 180)
					(length 2.54)
					(name "HIDRV")
					(number "18")
				)
				(pin passive line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "PHASE")
					(number "19")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 2.54)
					(name "VCC")
					(number "20")
				)
				(pin passive line
					(at 27.94 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
