(footprint "PG-TSON-8-3_6x5mm_P1.27mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.infineon.com/assets/row/public/packages/202/footprint_download/infineon-pg-tson-8-3-fpd-pdf-footprint-en.pdf")
	(tags "SMT")
	(property "Reference" "REF**"
		(at -4.89 -3.02 180)
		(layer "F.SilkS")
	)
	(property "Value" "PG-TSON-8-3_6x5mm_P1.27mm"
		(at -4.89 3.92 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at -5 10 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -4.89 5.12 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.89 6.32 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.89 7.52 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 270)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 270)
		(layer "User.9")
	)
	(pad "1" smd rect
		(at -2.75 -0.635 270)
		(size 3.08 1)
		(layers "F.Cu")
	)
	(pad "4" smd rect
		(at -2.75 1.905 270)
		(size 0.54 1)
		(layers "F.Cu")
	)
	(pad "8" smd rect
		(at 1 0 270)
		(size 4.45 4.5)
		(layers "F.Cu")
	)
	(embedded_fonts no)
	(model "antmicro_bsc021n08ns5atma1.glb"
		(offset
			(xyz -0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
