(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CSD86330Q3D"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CSD86330Q3D"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CSD86330Q3D"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/csd86330q3d.pdf?ts=1619602857581&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FCSD86330Q3D"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dual MOSFET, N Channel, 25 V, 25 V, 20 A, 20 A, 4.6 ohm"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CSD86330Q3D"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, IC, MOSFET, ARRAY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "DQZ8_1P8X2P7"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CSD86330Q3D_1_1"
				(pin passive line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "VIN")
					(number "1")
				)
				(pin passive line
					(at 12.7 2.54 180)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "2")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "TG")
					(number "3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TGR")
					(number "4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "BG")
					(number "5")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "VSW")
					(number "6")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VSW")
					(number "7")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VSW")
					(number "8")
				)
				(pin passive line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "PGND")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
