(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DMC2400UV-7"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DMC2400UV-7"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DMC2400UV-7"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/115/DIOD_S_A0010038249_1-2543538.pdf"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dual MOSFET, Complementary N and P Channel, 20 V, 20 V, 1.03 A, 1.03 A, 0.3 ohm"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DMC2400UV-7"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MOSFET, TRANSISTOR, ARRAY, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DMC2400UV-7_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "S1")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "G1")
					(number "2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D2")
					(number "3")
				)
				(pin passive line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "S2")
					(number "4")
				)
				(pin input line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "G2")
					(number "5")
				)
				(pin passive line
					(at 12.7 0 180)
					(length 2.54)
					(name "D1")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
