(footprint "PowerDI5060-8"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "PowerDI5060-8 (https://www.diodes.com/assets/Package-Files/PowerDI5060-8.pdf)")
	(tags "PowerDI5060-8")
	(property "Reference" "REF**"
		(at 0 -3.02 0)
		(layer "F.SilkS")
	)
	(property "Value" "PowerDI5060-8"
		(at -3.905 3.92 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.905 5.12 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.905 6.32 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.905 7.52 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(pad "1" smd roundrect
		(at -2.67 -1.905)
		(size 1.27 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(pad "2" smd roundrect
		(at -2.67 -0.635)
		(size 1.27 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(pad "3" smd roundrect
		(at -2.67 0.635)
		(size 1.27 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(pad "4" smd roundrect
		(at -2.67 1.905)
		(size 1.27 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(pad "5" smd roundrect
		(at -0.735 -2.05 90)
		(size 1.51 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08333333333)
	)
	(pad "5" smd roundrect
		(at -0.735 2.05 90)
		(size 1.51 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08333333333)
	)
	(pad "5" smd roundrect
		(at 0.69 0)
		(size 3.81 4.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.01312335958)
	)
	(pad "5" smd roundrect
		(at 1.69 -2.05 90)
		(size 1.51 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08333333333)
	)
	(pad "5" smd roundrect
		(at 1.69 2.05 90)
		(size 1.51 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08333333333)
	)
	(pad "5" smd roundrect
		(at 2.795 -1.905)
		(size 1.02 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(pad "5" smd roundrect
		(at 2.795 -0.635)
		(size 1.02 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(pad "5" smd roundrect
		(at 2.795 0.635)
		(size 1.02 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(pad "5" smd roundrect
		(at 2.795 1.905)
		(size 1.02 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08196721311)
	)
	(embedded_fonts no)
	(model "antmicro_dmp4015sps_13.glb"
		(offset
			(xyz -0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
