(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LED_RG_1204_KPBA-3010SURKMGKC_Horizontal"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LED_RG_1204_KPBA-3010SURKMGKC_Horizontal"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LED_RG_1204_KPBA-3010SURKMGKC_Horizontal"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/1854093.pdf?_gl=1*1onaj91*_gcl_aw*R0NMLjE3Mjc4NTYyMjYuQ2owS0NRanczdk8zQmhDcUFSSXNBRVdibGNCd3RaUkxTaXpPVWswNjdlZUhiM0NkMzV1X1E0X0tTWnlKR3Q2VTVBLXBvenFYOW9xb1g1Z2FBc1NzRUFMd193Y0I.*_gcl_au*MTIwOTQzNDEyMS4xNzI3NDE4MzEz"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LED, RG, SMD, 1204, R 20 mA, G 20 mA, R 1.95V, G 2.1V, Common Anode, Side Look"
				(at 27.94 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KPBA-3010SURKMGKC"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Kingbright"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Color" "R, G"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIODE, SEMICONDUCTOR, LED, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LED_RG_1204_KPBA-3010SURKMGKC_Horizontal_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "C_{G}")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "C_{R}")
					(number "2")
				)
				(pin passive line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "A")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
)
