(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT1738"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT1738"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT1738"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1738fa.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Slew Rate Controlled Ultralow Noise DC/DC Controller"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT1738EG#PBF"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT1738_1_1"
				(pin output line
					(at 21.59 -12.7 180)
					(length 2.54)
					(name "GATE")
					(number "1")
				)
				(pin output line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "CAP")
					(number "2")
				)
				(pin input line
					(at 21.59 0 180)
					(length 2.54)
					(name "GCL")
					(number "3")
				)
				(pin input line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "CS")
					(number "4")
				)
				(pin power_out line
					(at 0 -7.62 0)
					(length 2.54)
					(name "V5")
					(number "5")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SYNC")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CT")
					(number "7")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RT")
					(number "8")
				)
				(pin input line
					(at 21.59 -27.94 180)
					(length 2.54)
					(name "FB")
					(number "9")
				)
				(pin input line
					(at 21.59 -35.56 180)
					(length 2.54)
					(name "NFB")
					(number "10")
				)
				(pin power_in line
					(at 21.59 -40.64 180)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "VC")
					(number "12")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SS")
					(number "13")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "14")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "RCSL")
					(number "15")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RVSL")
					(number "16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "17")
				)
				(pin no_connect line
					(at 12.7 -43.18 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "18")
				)
				(pin no_connect line
					(at 8.89 -43.18 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "19")
				)
				(pin power_in line
					(at 21.59 -40.64 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
