(footprint "LQFN-16_2x3mm_P0.5mm_Analog-Devices_LTC4451"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.175 -2.398 0)
		(layer "F.SilkS")
	)
	(property "Value" "LQFN-16_2x3mm_P0.5mm_Analog-Devices_LTC4451"
		(at -13.325 0.227 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -13.325 4.002 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -13.325 5.202 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -13.325 6.402 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.9 -1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.9 -0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.9 -0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.9 0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.9 0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.9 1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.49 0.25)
		(size 0.725 2.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.25 1.4)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.25 1.4)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.49 0.25)
		(size 0.725 2.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.9 1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.9 0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.9 0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0.9 -0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0.9 -0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.9 -1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0.25 -1.4)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -0.25 -1.4)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_ltc4451av_trmpbf.glb"
		(offset
			(xyz 0 -0.002 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
