(footprint "LED_IR_LZ1-00R802"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "LED_IR_LZ1-00R802"
		(at 0 4.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -3.051 8.807 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.051 10.006 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.051 11.205 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.032 -2.085 180)
		(size 1.47 1.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.2)
		(chamfer top_left)
		(solder_mask_margin -0.12)
		(solder_paste_margin -0.12)
	)
	(pad "2" smd roundrect
		(at 2.08 -2.085 90)
		(size 1.47 1.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.2)
		(chamfer top_left)
		(solder_mask_margin -0.12)
		(solder_paste_margin -0.12)
	)
	(pad "3" smd roundrect
		(at 2.08 2.08)
		(size 1.47 1.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.2)
		(chamfer top_left)
		(solder_mask_margin -0.12)
		(solder_paste_margin -0.12)
	)
	(pad "4" smd roundrect
		(at -2.032 2.08 270)
		(size 1.47 1.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.2)
		(chamfer top_left)
		(solder_mask_margin -0.12)
		(solder_paste_margin -0.12)
	)
	(pad "5" smd circle
		(at 0.05 0.05 270)
		(size 3.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.15)
	)
	(embedded_fonts no)
	(model "antmicro_lz1_00r802_0000.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
