(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LED_IR_LZ1-00R802"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 25.4 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LED_IR_LZ1-00R802"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LED_IR_LZ1-00R802"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://dammedia.osram.info/media/resource/hires/osram-dam-20512286/LZ1-00R802_EN.pdf"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LED, Infrared (IR), SMD, 4-SMD, 1 A, 1.6 V, 1050 nm"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LZ1-00R802-0000"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "OSRAM"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Color" "IR"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIODE, SEMICONDUCTOR, LED"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LED_IR_LZ1-00R802_0_1")
			(symbol "LED_IR_LZ1-00R802_1_1"
				(text "~\n"
					(at 5.842 -2.794 900)
				)
				(text "~\n"
					(at 6.35 -2.794 900)
				)
				(text "~\n"
					(at 6.858 -2.794 900)
				)
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin input line
					(at 12.7 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin input line
					(at 12.7 0 180)
					(length 2.54)
					(hide yes)
					(name "")
					(number "3")
				)
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "")
					(number "4")
				)
				(pin input line
					(at 6.35 -6.35 90)
					(length 2.54)
					(name "5")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
