(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX16150A_SOT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 31.75 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX16150A_SOT"
				(at 31.75 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX16150A_SOT"
				(at 31.75 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX16150.pdf"
				(at 31.75 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pushbutton On/Off Controller, Latched Output, 1.3 to 5.5 V Supply, 50 ms Debounce Time, SOT-23-6"
				(at 31.75 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 31.75 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX16150AUT+T"
				(at 31.75 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "License" "Apache-2.0"
				(at 31.75 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 31.75 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, CONTROLLER, ESD, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX16150A_SOT_0_0"
				(text "CTRL"
					(at 8.89 -0.254 0)
				)
			)
			(symbol "MAX16150A_SOT_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{PB_IN}")
					(number "1")
				)
				(pin power_in line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin output line
					(at 17.78 0 180)
					(length 2.54)
					(name "OUT")
					(number "4")
				)
				(pin output line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "~{INT}")
					(number "5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{CLR}")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
