(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX33040_SOT23"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX33040_SOT23"
				(at 34.29 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX33040_SOT23"
				(at 34.29 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX33040E-MAX33041E.pdf"
				(at 34.29 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CAN Interface integrated circuit, 3V3-powered, 5Mbps CAN transceiver with 40V fault protection, 25V CMR and 40kV ESD in 8-Pin SOT23"
				(at 34.29 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX33040EAKA+T"
				(at 34.29 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 34.29 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, CAN, SMT, TRANSCEIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX33040_SOT23_1_1"
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TXD")
					(number "1")
				)
				(pin passive line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RXD")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SHDN")
					(number "5")
				)
				(pin passive line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "CANL")
					(number "6")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(name "CANH")
					(number "7")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "STBY")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
