(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX3373EEKA+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX3373EEKA+"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX3373EEKA+"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/en/products/max3373e.html"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "±15kV ESD-Protected, 1µA, 16Mbps, Dual/Quad Low-Voltage Level Translators in UCSP"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX3373EEKA+"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "LEVEL-SHIFTER, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX3373EEKA+_1_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "IO_V_{CC}2")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 2.54)
					(name "V_{L}")
					(number "3")
				)
				(pin bidirectional line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "IO_V_{L}2")
					(number "4")
				)
				(pin bidirectional line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "IO_V_{L}1")
					(number "5")
				)
				(pin input line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "~{THREE_STATE}")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IO_V_{CC}1")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
