(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MB10S"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MB10S"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MB10S"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.farnell.com/datasheets/2895435.pdf"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bridge Rectifier, 1000 V, 800 mA, Single Phase , 4 Pins, 1.1V"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MB10S"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Multicomp Pro"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, RECTIFIER, SEMICONDUCTOR, DIODE, BRIDGE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MB10S_1_1"
				(pin passive line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "4")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
