(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MPQ7235GQBE"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MPQ7235GQBE"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MPQ7235GQBE"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MPQ7235GQBE-AEC1/"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LED Driver, DC/DC, Synchronous Buck, 1.5 A, 1 Output, 2.2 MHz, AEC-Q100, QFN-13"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MPQ7235GQBE-AEC1-Z"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "LED, DRIVER, DC-DC , RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MPQ7235GQBE_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "2")
				)
				(pin no_connect line
					(at 17.78 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin output line
					(at 0 -13.97 0)
					(length 2.54)
					(name "~{FAULT}")
					(number "4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DIM")
					(number "5")
				)
				(pin passive line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "FB")
					(number "6")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "V_{CC}")
					(number "7")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "SW")
					(number "9")
				)
				(pin passive line
					(at 17.78 0 180)
					(length 2.54)
					(name "BST")
					(number "10")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
