(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NCV68061"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NCV68061"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NCV68061"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/ncv68061-d.pdf"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "OR Controller N+1 ORing Controller N-Channel 1:1 6-TSOP"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NCV68061SNAIT1G"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Onsemi"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONTROLLER, SEMICONDUCTOR, DIODE, PMOS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NCV68061_1_0"
				(pin no_connect line
					(at 12.7 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin passive line
					(at 15.24 0 180)
					(length 2.54)
					(name "G")
					(number "5")
				)
			)
			(symbol "NCV68061_1_1"
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin passive line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "D")
					(number "4")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "S")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
