(footprint "DFN-10_2.5x1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 1.524 -1.016 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-10_2.5x1mm"
		(at 2.032 1.524 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -0.95 3.524 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -0.95 4.724 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -0.95 5.924 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.425 -1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "2" smd roundrect
		(at -0.425 -0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "3" smd roundrect
		(at -0.425 0 270)
		(size 0.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "4" smd roundrect
		(at -0.425 0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "5" smd roundrect
		(at -0.425 1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "6" smd roundrect
		(at 0.425 1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "7" smd roundrect
		(at 0.425 0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "8" smd roundrect
		(at 0.425 0 270)
		(size 0.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "9" smd roundrect
		(at 0.425 -0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "10" smd roundrect
		(at 0.425 -1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_pesd4usb5u_tts.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
