(footprint "Nexperia_DFN-10_2.5x1mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.016 -0.995 0)
		(layer "F.SilkS")
	)
	(property "Value" "Nexperia_DFN-10_2.5x1mm_P0.5mm"
		(at -0.016 1.705 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.367 3.704 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.367 4.905 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.367 6.105 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1 0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "2" smd rect
		(at -0.5 0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "3" smd rect
		(at 0 0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "4" smd rect
		(at 0.5 0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "5" smd rect
		(at 1 0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "6" smd rect
		(at 1 -0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "7" smd rect
		(at 0.5 -0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "8" smd rect
		(at 0 -0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "9" smd rect
		(at -0.501 -0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "10" smd rect
		(at -1 -0.3875)
		(size 0.2 0.475)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_pusb3f96x.glb"
		(offset
			(xyz -1.01553 -1.905708 1.45)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
