(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PUSB3F96X_PASS"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "D"
				(at 25.4 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PUSB3F96X_PASS"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PUSB3F96X_PASS"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mouser.com/datasheet/2/916/PUSB3F96-1600324.pdf"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "TVS diode array, 10 kV, DFN-2510, 5.5 V, 0.5 pF"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nexperia"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PUSB3F96X"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIODE, SEMICONDUCTOR, TVS, ESD, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PUSB3F96X_PASS_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "CH1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "CH2")
					(number "2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CH3")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CH4")
					(number "5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "CH4")
					(number "6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "CH3")
					(number "7")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "CH2")
					(number "9")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "CH1")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
