(footprint "Vishay_PowerPAK_1212-8_Dual"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "PowerPAK 1212-8 Dual (https://www.vishay.com/docs/71656/ppak12128.pdf, https://www.vishay.com/docs/72598/72598.pdf)")
	(tags "Vishay_PowerPAK_1212-8_Dual")
	(property "Reference" "REF**"
		(at 0 -2.159 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vishay_PowerPAK_1212-8_Dual"
		(at 0 2.794 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.94 4.675 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.94 5.875 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.94 7.075 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.449 -0.975)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
	)
	(pad "2" smd roundrect
		(at -1.449 -0.325)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
	)
	(pad "3" smd roundrect
		(at -1.449 0.324)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
	)
	(pad "4" smd roundrect
		(at -1.449 0.975)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
	)
	(pad "5" smd roundrect
		(at -0.2 0.95 180)
		(size 0.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(zone_connect 2)
	)
	(pad "5" smd roundrect
		(at 0.45 0.65 180)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
		(zone_connect 2)
	)
	(pad "5" smd roundrect
		(at 1.45 0.325 180)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
		(zone_connect 2)
	)
	(pad "5" smd roundrect
		(at 1.45 0.975 180)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
		(zone_connect 2)
	)
	(pad "6" smd roundrect
		(at -0.2 -0.95)
		(size 0.4 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(zone_connect 2)
	)
	(pad "6" smd roundrect
		(at 0.45 -0.65)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
		(zone_connect 2)
	)
	(pad "6" smd roundrect
		(at 1.45 -0.975)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
		(zone_connect 2)
	)
	(pad "6" smd roundrect
		(at 1.45 -0.325)
		(size 0.56 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1219512195)
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "antmicro_si7223dn_t1_ge3.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
