(footprint "antmicro_sqs401en_t1_be3"
  (version 20240108) (generator "partreel")
  (layer "F.Cu")
  (descr "Vishay_PowerPAK_1212-8_Single replacement land pattern per manufacturer datasheet: Vishay AN826 (doc 72597, rev 2008-01-21) p.7 recommended minimum pads; dimensions re-measured from the PDF vector geometry (agreement within 0.005mm); drain modeled as thermal rect + 4 merged lead tabs per the drawing")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.1) (layer "F.SilkS"))
  (fp_text value "VAL**" (at 0 3.1) (layer "F.Fab"))
  (pad "1" smd rect (at -1.436 -0.99) (size 0.99 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.436 -0.33) (size 0.99 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.436 0.33) (size 0.99 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -1.436 0.99) (size 0.99 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 0.559 0) (size 1.725 2.235) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 1.5495 -0.99) (size 0.76 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 1.5495 -0.33) (size 0.76 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 1.5495 0.33) (size 0.76 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 1.5495 0.99) (size 0.76 0.405) (layers "F.Cu" "F.Paste" "F.Mask"))
)
