(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPD8S009DSMR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPD8S009DSMR"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPD8S009DSMR"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tpd8s009.pdf?ts=1679406571326&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTPD8S009%252Fpart-details%252FTPD8S009DSMR"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "TVS diode array, 8 kV, R-PDSO-N15, 5.5 V, 0.8 pF"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPD8S009DSMR"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIODE, SEMICONDUCTOR, TVS, ESD, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPD8S009DSMR_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "D0+")
					(number "1")
				)
				(pin passive line
					(at 16.51 -17.78 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "D0-")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "D1+")
					(number "4")
				)
				(pin passive line
					(at 16.51 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D1-")
					(number "6")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D2+")
					(number "7")
				)
				(pin passive line
					(at 16.51 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D2-")
					(number "9")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D3+")
					(number "10")
				)
				(pin passive line
					(at 16.51 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D3-")
					(number "12")
				)
				(pin power_in line
					(at 16.51 0 180)
					(length 2.54)
					(name "VCC")
					(number "13")
				)
				(pin no_connect line
					(at 13.97 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin passive line
					(at 16.51 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "15")
				)
			)
			(embedded_fonts no)
		)
)
