(footprint "VQFN-HR-10_2x2mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-HR-10_2x2mm"
		(at -1.45 2.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 -0.045 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "RPW0010A"
		(at -1.45 3.65 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.45 4.85 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.45 6.05 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.45 7.25 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.9 -0.6875)
		(size 0.6 0.275)
		(layers "F.Paste")
		(roundrect_rratio 0.1818181818)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.9 0.6875)
		(size 0.6 0.275)
		(layers "F.Paste")
		(roundrect_rratio 0.1818181818)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.7125 -0.875)
		(size 0.225 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.2222222222)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.7125 0.875)
		(size 0.225 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.2222222222)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.25 -0.63)
		(size 0.28 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.25 0.63)
		(size 0.28 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 0.25 -0.63)
		(size 0.28 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 0.25 0.63)
		(size 0.28 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 0.7125 -0.875)
		(size 0.225 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.2222222222)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 0.7125 0.875)
		(size 0.225 0.65)
		(layers "F.Paste")
		(roundrect_rratio 0.2222222222)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 0.9 -0.6875)
		(size 0.6 0.275)
		(layers "F.Paste")
		(roundrect_rratio 0.1818181818)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 0.9 0.6875)
		(size 0.6 0.275)
		(layers "F.Paste")
		(roundrect_rratio 0.1818181818)
		(thermal_bridge_angle 45)
	)
	(pad "1" smd roundrect
		(at -0.9 -0.7)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "1" smd roundrect
		(at -0.725 -0.875 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -0.9 -0.225)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -0.9 0.225)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -0.9 0.7)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -0.725 0.875 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -0.25 0)
		(size 0.3 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 0.25 0)
		(size 0.3 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 0.725 0.875 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 0.9 0.7 180)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 0.9 0.225 180)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at 0.9 -0.225 180)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 0.725 -0.875 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 0.9 -0.7 180)
		(size 0.6 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "antmicro_tps259474arpwr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
