(footprint "VQFN-24-1EP_4x4x1mm_P0.5mm_EP2.7x2.7mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Texas Instruments RGE 24 (https://www.ti.com/lit/ml/mpqf124g/mpqf124g.pdf)")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-24-1EP_4x4x1mm_P0.5mm_EP2.7x2.7mm"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.503 5.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.503 6.6 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.503 7.8 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.7 -0.7)
		(size 1.18 1.18)
		(layers "F.Paste")
		(roundrect_rratio 0.08474576271)
	)
	(pad "" smd roundrect
		(at -0.7 0.7)
		(size 1.18 1.18)
		(layers "F.Paste")
		(roundrect_rratio 0.08474576271)
	)
	(pad "" smd roundrect
		(at 0.7 -0.7)
		(size 1.18 1.18)
		(layers "F.Paste")
		(roundrect_rratio 0.08474576271)
	)
	(pad "" smd roundrect
		(at 0.7 0.7)
		(size 1.18 1.18)
		(layers "F.Paste")
		(roundrect_rratio 0.08474576271)
	)
	(pad "1" smd roundrect
		(at -1.915 -1.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "2" smd roundrect
		(at -1.915 -0.75)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "3" smd roundrect
		(at -1.915 -0.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "4" smd roundrect
		(at -1.915 0.248)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "5" smd roundrect
		(at -1.915 0.748)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "6" smd roundrect
		(at -1.915 1.249)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "7" smd roundrect
		(at -1.25 1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "8" smd roundrect
		(at -0.75 1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "9" smd roundrect
		(at -0.25 1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "10" smd roundrect
		(at 0.248 1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "11" smd roundrect
		(at 0.748 1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "12" smd roundrect
		(at 1.249 1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "13" smd roundrect
		(at 1.915 1.249)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "14" smd roundrect
		(at 1.915 0.748)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "15" smd roundrect
		(at 1.915 0.248)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "16" smd roundrect
		(at 1.915 -0.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "17" smd roundrect
		(at 1.915 -0.75)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "18" smd roundrect
		(at 1.915 -1.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "19" smd roundrect
		(at 1.249 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "20" smd roundrect
		(at 0.748 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "21" smd roundrect
		(at 0.248 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "22" smd roundrect
		(at -0.25 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "23" smd roundrect
		(at -0.75 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "24" smd roundrect
		(at -1.25 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "25" smd roundrect
		(at 0 0)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.01851851852)
	)
	(embedded_fonts no)
	(model "antmicro_tps26631rger.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
