(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS26631RGER"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS26631RGER"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS26631RGER"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2663.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "4.5-V to 60-V, 31mΩ, 0.6-6A eFuse with output power limiting and surge protection, -40 to 125 Deg C"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS26631RGER"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONTROLLER, IC, DIODE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS26631RGER_1_1"
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "B_GATE")
					(number "3")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DRV")
					(number "4")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "IN_SYS")
					(number "5")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "UVLO")
					(number "6")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "OVP")
					(number "7")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 3.81)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 25.4 -35.56 180)
					(length 3.81)
					(name "dVdT")
					(number "9")
				)
				(pin passive line
					(at 25.4 -33.02 180)
					(length 3.81)
					(name "ILIM")
					(number "10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "MODE")
					(number "11")
				)
				(pin passive line
					(at 25.4 -27.94 180)
					(length 3.81)
					(name "~{SHDN}")
					(number "12")
				)
				(pin passive line
					(at 25.4 -30.48 180)
					(length 3.81)
					(name "IMON")
					(number "13")
				)
				(pin passive line
					(at 25.4 -25.4 180)
					(length 3.81)
					(name "~{FLT}")
					(number "14")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 3.81)
					(name "PGTH")
					(number "15")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 3.81)
					(name "PGOOD")
					(number "16")
				)
				(pin no_connect line
					(at 21.59 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "19")
				)
				(pin no_connect line
					(at 21.59 -11.43 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin no_connect line
					(at 21.59 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "21")
				)
				(pin no_connect line
					(at 21.59 -13.97 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "22")
				)
				(pin no_connect line
					(at 21.59 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "23")
				)
				(pin no_connect line
					(at 21.59 -16.51 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "24")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 3.81)
					(name "EP")
					(number "25")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "IN")
					(number "[1,2]")
				)
				(pin power_out line
					(at 25.4 0 180)
					(length 3.81)
					(name "OUT")
					(number "[17,18]")
				)
			)
			(embedded_fonts no)
		)
)
