(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS25200DRVR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS25200DRVR"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS25200DRVR"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Ftps25200"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "6.5 V/2.8 A eFuse with Overvoltage Clamp"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS25200DRVR"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, SWITCH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS25200DRVR_1_1"
				(pin power_out line
					(at 16.51 0 180)
					(length 2.54)
					(name "OUT")
					(number "1")
				)
				(pin output line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "ILIM")
					(number "2")
				)
				(pin output line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "~{FAULT}")
					(number "3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "4")
				)
				(pin power_in line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "EP")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
)
