(footprint "FUSC_AVX_F0603G"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "0603 (1608mm), Body 1.60 x .81mm, Fast Acting Chip Fuse")
	(property "Reference" "REF**"
		(at 0 -1.525 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSC_AVX_F0603G"
		(at 0 1.525 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -0.775 0)
		(size 0.85 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.775 0)
		(size 0.85 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
