(footprint "FUSH_BUSSMANN_1A3400-09"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "BUSSMANN 1A3400-09, Fuse holder for 10x38mm Fuses")
	(property "Reference" "REF**"
		(at 0 -6.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSH_BUSSMANN_1A3400-09"
		(at 0 6.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at -4.85 0)
		(size 2.9 2.9)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 11 11)
		(drill 3.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 5.5 5.5)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 5.5 5.5)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 4.85 0)
		(size 2.9 2.9)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
