(footprint "FUSH_EATON_HTC-100M"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuse Holder for 10.3x38mm (5AG) Fuses, Body L 43.05 x W 18.14 x H 17.53mm")
	(property "Reference" "REF**"
		(at 0 -5.675 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSH_EATON_HTC-100M"
		(at 0 5.675 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" thru_hole circle
		(at -11.3 0)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 11.3 0)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
