(footprint "FUSH_KEYSTONE_4245"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "KEYSTONE 4245, Fuse holder for 6..3x32mm Fuses")
	(property "Reference" "REF**"
		(at 0 -4.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSH_KEYSTONE_4245"
		(at 0 4.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at -17.46251 0)
		(size 2.4 2.4)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "1" smd rect
		(at -13.65251 0)
		(size 8 7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -4)
		(solder_paste_margin -4)
	)
	(pad "1" thru_hole circle
		(at -9.84251 0)
		(size 2.4 2.4)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 9.84251 0)
		(size 2.4 2.4)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" smd rect
		(at 13.65251 0)
		(size 8 7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -4)
		(solder_paste_margin -4)
	)
	(pad "2" thru_hole circle
		(at 17.46251 0)
		(size 2.4 2.4)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
