(footprint "FUSH_SCHURTER_0031.8231"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SCHURTER OGD Series, Fuse holder for 5x20mm/6.3x32mm Fuses")
	(property "Reference" "REF**"
		(at 0.00004 -6.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSH_SCHURTER_0031.8231"
		(at 0.00004 6.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at -9.99996 -2.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole circle
		(at -9.99996 2.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 10.00005 -2.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 10.00005 2.5)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 0.00004 0)
		(size 4.5 4.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
