(footprint "FUSH_SCHURTER_3101.0050"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SCHURTER Type FPG5, Horizontal Fuse holder for 5x20mm Fuses")
	(property "Reference" "REF**"
		(at -14.25001 -7.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSH_SCHURTER_3101.0050"
		(at -14.25001 7.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "" np_thru_hole circle
		(at -20.32001 0)
		(size 0.5 0.5)
		(drill 2)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.75)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole circle
		(at 0 -2.54)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole circle
		(at 0 2.54)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -7.62001 0)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
