(footprint "FUSR_LITTELFUSE_MICROSMD005F"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PolySwitch Resettable PPTC, 2-Leads, Body 3.22mm x 2.57mm Nominal")
	(property "Reference" "REF**"
		(at 0 -2.375 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSR_LITTELFUSE_MICROSMD005F"
		(at 0 2.375 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -1.5 0)
		(size 1 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.5 0)
		(size 1 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.8 -1.4) (xy 0.8 -1.4) (xy 0.8 1.4) (xy -0.8 1.4)
			)
		)
	)
	(embedded_fonts no)
)
