(footprint "FUSR_BUSSMANN_PTS181216V035"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1812 (4532mm), Body 4,40 x 3.24mm, Surface Mount PTC Resettable Fuse, PTS Series")
	(property "Reference" "REF**"
		(at 0.0015 -2.725 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSR_BUSSMANN_PTS181216V035"
		(at 0.0015 2.725 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -2.615 0)
		(size 1.78 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.615 0)
		(size 1.78 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
