(footprint "SAR_TDK_A80-C90XSMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Surge Arrester,Axial Diameter, D8.3mm x L 6.25mm")
	(property "Reference" "REF**"
		(at 0 -5.125 0)
		(layer "F.SilkS")
	)
	(property "Value" "SAR_TDK_A80-C90XSMD"
		(at 0 5.125 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -3.025 0)
		(size 1.35 4.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.025 0)
		(size 1.35 4.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
