(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "24AA32AT-I_TDFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "24AA32AT-I_TDFN"
				(at 38.1 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "24AA32AT-I_TDFN"
				(at 38.1 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/268/24AA32A_24LC32A_32_Kbit_I2C_Serial_EEPROM_20001713-2898696.pdf"
				(at 38.1 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "EEPROM Memory IC 32Kbit I²C 400 kHz 900 ns 8-TDFN (2x3)"
				(at 38.1 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "24AA32AT-I/MNY"
				(at 38.1 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 38.1 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, MEMORY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "24AA32AT-I_TDFN_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "A0")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin input line
					(at 15.24 -7.62 180)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin input line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "WP")
					(number "7")
				)
				(pin power_in line
					(at 15.24 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
