(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "24LC02BT-I-SN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "24LC02BT-I-SN"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "24LC02BT-I-SN"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/24AA02-24LC02B-24FC02-2K-I2C-Serial-EEPROM-20001709N.pdf"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "EEPROM, 2 Kbit, 256 x 8bit, Serial I2C (2-Wire), 2.5V-5.5V, 8 Fixed I2C Addreses, 400 kHz, SOIC-8, 5 Pins"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "24LC02BT-I/SN"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "EEPROM, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "24LC02BT-I-SN_1_1"
				(pin no_connect line
					(at 12.7 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "A0")
					(number "1")
				)
				(pin no_connect line
					(at 12.7 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "A1")
					(number "2")
				)
				(pin no_connect line
					(at 12.7 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "A2")
					(number "3")
				)
				(pin power_in line
					(at 15.24 -6.35 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at 15.24 0 180)
					(length 2.54)
					(name "WP")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
