(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "24LC32AT-E-MC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "24LC32AT-E-MC"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "24LC32AT-E-MC"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/21713M-243047.pdf"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "EEPROM, 32 Kbit, 4k x 8bit, Serial I2C (2-Wire), TDFN, 8 Pins"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "24LC32AT-E/MC"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "EEPROM, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "24LC32AT-E-MC_1_1"
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A0")
					(number "1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin passive line
					(at 16.51 -15.24 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "WP")
					(number "7")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin passive line
					(at 16.51 -12.7 180)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
