(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "W25Q16FW_WSON-8"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 36.83 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "W25Q16FW_WSON-8"
				(at 36.83 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "W25Q16FW_WSON-8"
				(at 36.83 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.winbond.com/hq/support/documentation/downloadV2022.jsp?__locale=en&xmlPath=/support/resources/.content/item/DA00-W25Q16FW.html&level=1"
				(at 36.83 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "16M-bit 1.8V Serial Flash Memory with uniform 4KB sectors and Dual/Quad SPI and QPI"
				(at 37.084 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "25Q16FWIQ"
				(at 36.83 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Winbond"
				(at 36.83 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 37.084 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, SPI, FLASH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "W25Q16FW_WSON-8_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SO(IO1)")
					(number "2")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{WP(IO2})")
					(number "3")
				)
				(pin power_in line
					(at 24.13 -12.7 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SI(IO0)")
					(number "5")
				)
				(pin input clock
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCLK")
					(number "6")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{HOLD(IO3})")
					(number "7")
				)
				(pin power_in line
					(at 24.13 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin no_connect line
					(at 21.59 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
