(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74HC00_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74HC00_TSSOP"
				(at 27.94 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74HC00_TSSOP"
				(at 27.94 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT00.pdf"
				(at 27.94 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NAND Gate IC 4 Channel 14-TSSOP"
				(at 27.94 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nexperia"
				(at 27.94 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74HC00PW,118"
				(at 27.94 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 27.94 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "GATE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74HC00_TSSOP_1_1"
				(text "4xNAND"
					(at 3.81 -13.97 0)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "1A")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "1B")
					(number "2")
				)
				(pin passive line
					(at 15.24 -3.81 180)
					(length 2.54)
					(name "~{1Y}")
					(number "3")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "2A")
					(number "4")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 2.54)
					(name "2B")
					(number "5")
				)
				(pin passive line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "~{2Y}")
					(number "6")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin passive line
					(at 15.24 -16.51 180)
					(length 2.54)
					(name "~{3Y}")
					(number "8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "3A")
					(number "9")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "3B")
					(number "10")
				)
				(pin passive line
					(at 15.24 -22.86 180)
					(length 2.54)
					(name "~{4Y}")
					(number "11")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 2.54)
					(name "4A")
					(number "12")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 2.54)
					(name "4B")
					(number "13")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
