(footprint "TSSOP-20_W4.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "http://www.ti.com/lit/ds/symlink/txb0108.pdf")
	(property "Reference" "REF**"
		(at -3.91 -3.83 0)
		(layer "F.SilkS")
	)
	(property "Value" "TSSOP-20_W4.4mm"
		(at -5.33 4.57 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.33 6.57 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.33 7.77 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.33 8.97 0)
		(layer "F.Fab")
	)
	(fp_text user "REF**"
		(at -5.33 10.17 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.926 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "2" smd rect
		(at -2.275 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "3" smd rect
		(at -1.625 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "4" smd rect
		(at -0.975 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "5" smd rect
		(at -0.328 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "6" smd rect
		(at 0.325 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "7" smd rect
		(at 0.972 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "8" smd rect
		(at 1.624 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "9" smd rect
		(at 2.273 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "10" smd rect
		(at 2.922 2.797)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "11" smd rect
		(at 2.922 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "12" smd rect
		(at 2.273 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "13" smd rect
		(at 1.624 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "14" smd rect
		(at 0.972 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "15" smd rect
		(at 0.325 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "16" smd rect
		(at -0.328 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "17" smd rect
		(at -0.975 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "18" smd rect
		(at -1.625 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "19" smd rect
		(at -2.275 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "20" smd rect
		(at -2.926 -2.801)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(embedded_fonts no)
	(model "antmicro_74hc688pw_118.glb"
		(offset
			(xyz -2.925 -3.2 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
