(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74HC688PW"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74HC688PW"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74HC688PW"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC688.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8-bit magnitude comparator"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nexperia"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74HC688PW,118"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, GATE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74HC688PW_1_1"
				(text ""
					(at 2.54 -3.048 0)
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "~{E}")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "P0")
					(number "2")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "Q0")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "P1")
					(number "4")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "Q1")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "P2")
					(number "6")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "Q2")
					(number "7")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "P3")
					(number "8")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "Q3")
					(number "9")
				)
				(pin power_in line
					(at 20.32 -50.8 180)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "P4")
					(number "11")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "Q4")
					(number "12")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "P5")
					(number "13")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "Q5")
					(number "14")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "P6")
					(number "15")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "Q6")
					(number "16")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "P7")
					(number "17")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "Q7")
					(number "18")
				)
				(pin output line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "~{P=Q}")
					(number "19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
